**Vlan Setup on Switch:**

**Name vlan**

En > config T > Vlan # > name VlanName

**Verify vlan**

Show vlan brief

**Set access mode:**

En > config t> interface Port# > switchport mode access/trunk

**Set access mode for Vlan:**

En > config t> interface Port# > switchport access vlan#

NAT

Create pool

Access list

Port

permit

ip nat inside source static “one port ip address” (to) “other port ip address”